EPIC GUIDE SPECIFICATION
SECTION 09 72 00
ARCHITECTURAL FINISH FILM WALL COVERINGS (3M™ DI-NOC™)
Basis of design and installation standard: Epic Security & Architectural Window Films and Graphics (Epic Solar Control, LLC). Revision October 2026.
3255 N McDonald St, Suite 1, McKinney, TX 75071 · 16302 E 2nd Ave, Suite 160, Aurora, CO 80011
866.EPIC.117 (866.374.2117) · sales@epiccos.com · epiccos.com
3M™ Platinum Elite National Dealer · 100% woman-owned · Certified Installation Specialists are Epic employees, never subcontracted
[SPECIFIER NOTE: This guide specification is written in CSI three-part format for insertion into a project manual. Bracketed, italic text is a specifier note or a choice to be made; delete the notes and unused options before issue. Product values are the manufacturer’s published data for the representative shade on 1/4 in. clear glass and are subject to the manufacturer’s current literature. Epic will review a draft section at no charge and return it marked for the project’s glass, frames and threat or performance criteria: sales@epiccos.com.]
PART 1 — GENERAL
1.1  SUMMARY
A.	Section includes: self-adhesive architectural finish film applied over existing or new interior surfaces — walls, columns, doors, elevator cab interiors and doors, casework, millwork, reception desks and ceilings — to produce wood, stone, metal, textile, leather, solid-colour and abstract finishes without demolition, installed by a manufacturer-trained and certified installer.
B.	Related sections: Section 09 29 00 Gypsum Board; Section 14 21 00 Electric Traction Elevators (cab finish coordination); Section 08 87 26 Decorative Glass Film.
1.2  REFERENCES
A.	ASTM E84 — Surface Burning Characteristics of Building Materials (pattern-specific report required in the submittal).
B.	Manufacturer’s current product bulletin, application guide and primer guide for the specified series.
1.3  SUBMITTALS
A.	Product data and pattern-specific ASTM E84 report for each pattern; 4 × 6 in. physical sample of each pattern; where available, a wrapped sample on the project’s substrate profile.
B.	Shop drawings: each surface at scale with pattern direction, seam locations, terminations, returns, reveals and edge treatment; elevator cab drawings coordinated with the elevator contractor.
C.	Installer certification per Article 1.4; substrate preparation and primer schedule by substrate; mock-up approval.
D.	Closeout: as-installed record by surface, pattern numbers and roll lots, care instructions, manufacturer’s warranty registration.
1.4  QUALITY ASSURANCE
A.	Installer: trained and certified by the film manufacturer for architectural finish film, a 3M™ Platinum Elite National Dealer, with installation personnel who are direct employees of the Installer; no subcontracted installation labor. [Specifier note: the manufacturer’s warranty on finish film is conditioned on certified installation.]
B.	Mock-up: one 4 × 4 ft. field area and one of each detail condition (outside corner, inside corner, reveal, door edge, cab return) for each pattern, approved before proceeding.
C.	Pattern direction, seam placement and returns shall match the approved shop drawings; visible seams shall be located at natural breaks and shall not occur mid-panel on a focal surface.
1.5  WARRANTY
A.	Manufacturer’s warranty for interior vertical applications of the specified series, up to 12 years per the manufacturer’s current bulletin, registered by the Installer; horizontal, exterior and high-traffic applications per the series bulletin. Installer’s workmanship warranty for the same term.
PART 2 — PRODUCTS
2.1  MANUFACTURERS AND INSTALLER
A.	Basis of design: 3M™ DI-NOC™ Architectural Finishes, 3M Company, St. Paul, MN; installed by Epic Security & Architectural Window Films and Graphics (Epic Solar Control, LLC), McKinney, TX and Aurora, CO; 866.374.2117; sales@epiccos.com.
B.	Substitutions: not permitted without pattern-specific samples, fire data and a certified installer named at bid. [Specifier note: delete if substitutions are not permitted.]
2.2  ARCHITECTURAL FINISH FILM
	Series family
	Typical use
	Schedule

	Fine Wood / Wood Grain / Dry Wood / Premium Wood
	Walls, doors, cabs, casework
	Pattern no. ____

	Metallic / Hairline / Advanced Metallic / Aged Metal
	Elevator doors and returns, reception fronts, columns
	Pattern no. ____

	Stone / Abstract Earth / Concrete / Sand
	Lobby walls, cab panels, feature walls
	Pattern no. ____

	Single Color / Textile / Leather / Suede
	Corridors, offices, millwork, soffits
	Pattern no. ____

	Exterior-rated series (EX)
	Entrances, storefront fascia, exterior columns
	Pattern no. ____



A.	Film: 3M™ DI-NOC™ Architectural Finish, series and pattern as scheduled, nominal 8 mil, with the manufacturer’s pressure-sensitive, air-release adhesive; ASTM E84 Class A per the pattern report.
B.	Primer and accessories: the manufacturer’s specified primer for each substrate (gypsum, metal, laminate, wood, existing finish), edge sealer where scheduled, and the manufacturer’s approved application tools. [Specifier note: Quick Ship patterns are stocked by 3M for short lead times; Epic will mark the schedule accordingly.]
PART 3 — EXECUTION
3.1  EXAMINATION AND SUBSTRATE PREPARATION
A.	Examine each substrate for flatness, soundness, moisture and contamination. Fill, sand and seal as required to the manufacturer’s surface standard (finish film telegraphs every defect); prime per the primer schedule; allow full cure before application. Remove or mask hardware; coordinate elevator cab work with the elevator contractor and the Owner’s shutdown schedule.
3.2  APPLICATION
A.	Apply with the manufacturer’s dry method, heat-forming at corners, returns and profiles to the manufacturer’s temperature and post-heat requirements; seams butted or overlapped per the pattern bulletin at the locations shown; returns wrapped not less than 1/4 in. and sealed where scheduled. No lifting, bridging, bubbles, pattern misalignment or visible adhesive.
3.3  FIELD QUALITY CONTROL, RECORD AND CARE
A.	Walk every surface with the Owner at completion; touch up and replace panels that do not meet the approved mock-up. Deliver the as-installed record by surface with pattern numbers and roll lots, and the manufacturer’s care instructions. Register the warranty within 30 days.
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